CHxx_VIDEO_CTRL

CHxx_VIDEO_TCP_IP, CHxx_VIDEO_MULTICAST_IP

Description

> Set or Get the IP and Multicast IP addresses of the encoder for the decoder.

> In CHxx_VIDEO_TCP_IP URL, it sets the encoder's IP address to the decoder for the connection.

> In CHxx_VIDEO_MULTICAST_IP URL, it sets the encoder's multicast IP address to the decodeer.

Input Argument

> IPv4 unicast or multicast address

Attribute

- Write Only in WPL Decoders
- Readable and Writable in EPL Decoders
- Not On-Fly

Return of Message

> In WPL Decoder Devices

> - None

> In EPL Decoder Devices

> - Read Operation

> > CH01_VIDEO_TCP_IP='192.168.0.100'
> > CH01_VIDEO_MULTICAST_IP='228.5.6.1'

> - Write Operation

> > OK: CH01_VIDEO_TCP_IP='192.168.0.100'
> > OK: CH01_VIDEO_MULTICAST_IP='228.5.6.1'
> > or
> > ERROR: CH01_VIDEO_TCP_IP='192.168.0.100'
> > ERROR: CH01_VIDEO_MULTICAST_IP='228.5.6.1'

Applicability

- WPL Decoder Devices
- EPL Decoder Devices

Status

> Valid

See Also

> CHxx_VIDEO_CONNECT, CHxx_VIDEO_VARFPS, CHxx_VIDEO_STREAM, CHxx_VIDEO_AUDIO, CHxx_VIDEO_CONTROL, CHxx_VIDEO_USERNAME, CHxx_VIDEO_PASSWORD, CHxx_PORT_STREAM, CHxx_PORT_CONTROL, CHxx_PORT_MULTICAST, CHxx_PORT_RTP, CHxx_PORT_HTTP, CHxx_TIME, CHxx_SOURCE_TYPE, CHxx_QUAD_CHANNEL, CHxx_CHANNEL, SWITCH, VIDEO_VARFPS

Example

- Read Operation (Only in EPL Decoder Devices)

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CH01_VIDEO_TCP_IP
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CH01_VIDEO_MULTICAST_IP

- Write Operation

> In WPL Decoder Devices

> > http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CHxx_VIDEO_TCP_IP=192.168.0.100
> > http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CHxx_VIDEO_MULTICAST_IP=228.5.6.1
> > where xx is from 01~16

> In EPL Decoder Devices

> > http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CH01_VIDEO_TCP_IP=192.168.0.100
> > http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CH01_VIDEO_MULTICAST_IP=228.5.6.1

Back to

> HOME, URL CGI