TOS_PRIORITY

VIDEO_TOS_PRIOIRTY

Description

> Get or Set ToS (Type of Service) priority configuration. The ToS setting will be set to the ToS field in IP header of every video and audio packet.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNLE 1 video server's TOS configurations will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> Minimize-Delay, Maximize-Throughput, Maximize-Reliability, Normal-Service

Attribute

- Readable and Writable (except all devices in Multi-Channel Platform)
- On-Fly (except all encoders in WPL Platform)

Return of Message

- Read Operation

> VIDEO_TOS_PRIORITY='Normal-Service'

- Write Operation

> OK: VIDEO_TOS_PRIORITY='Normal-Service'
> or
> ERROR: VIDEO_TOS_PRIORITY='Normal-Service'

Applicability

- WPL Platform : All Encoder Devices
- EPL Platform : All Encoder Devices
- PlatformT : All encoder Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> VIDEO_TOS, VIDEO_TOS_TYPE

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&VIDEO_TOS_PRIORITY
> or
> http://ip:port/cgi-bin/cmd/system?VIDEO_TOS_PRIORITY

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&VIDEO_TOS_PRIORITY=Normal-Service
> or
> http://ip:port/cgi-bin/cmd/system?VIDEO_TOS_PRIORITY=Normal-Service

Back to

> HOME, SYSTEM CGI