V2_MULTICAST_IP

Description

> Get or Set the multicast IP address configuration.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, it will set the base of the multicast IP address of all channels. The multicast IP address of CHNNAEL n will be the base multicast IP address + n -1. For example, the VIDEO_MULTICAST_IP=228.5.6.1 sets the multicast IP address of CHANNEL 1 to be 228.5.6.1 and the multicast IP address of CHANNEL 2 to be 228.5.6.2.

Input Argument

> IPv4 Multicast Address.

Attribute

- Readable and Writable
- On-Fly (except all encoders in WPL and Multi-Channel Platforms)

Return of Message

- Read Operation

> V2_MULTICAST_TTL='228.5.6.1'

- Write Operation

> OK: V2_MULTICAST_TTL='228.5.6.1'
> or
> ERROR: V2_MULTICAST_TTL='228.5.6.1'

Applicability

- WPL Platform : All encoder Devices
- EPL Platform : All encoder Devices
- PlatformT : All encoder Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> PORT_MULTICAST, V2_PORT_RTP_MULTI_VIDEO, V2_PORT_RTP_MULTI_AUDIO, VIDEO_MULTICAST_TTL, V2_MULTICAST_IF, IGMP_ENABLED

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_MULTICAST_IP
> or
> http://ip:port/cgi-bin/cmd/system?V2_MULTICAST_IP

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_MULTICAST_IP=228.5.6.1
> or
> http://ip:port/cgi-bin/cmd/system?V2_MULTICAST_IP=228.5.6.1

Back to

> HOME, SYSTEM CGI