URL Command Specification Version

URL Command Specification

VERSION V2.0.05

Version | Date | Description

V2.0.00

2007/11/23

- Document created

V2.0.01

2007/12/26

- Add Description of URL, Return Message sections

V2.0.02

2008/01/03

- Add UPDATE CGI, URL CGI and QUAD CGI, ACTIVEX_URL and FW_UPG_STATUS in SYSTEM CGI
- Correct the DIO_STATUS URL in MPEG4 CGI
- Add the Daylight Saving Design Specification and Camera Doctor Design Specification

V2.0.03

2008/01/24

- Change the MOTION_CONFIG, MOTION_CONFIG_GET URLs in ENCODER CGI
- MOTION_OBJ and SNAPSHOT URLs in ENCODER CGI
- Add "invalid parameters" error message in the return of URL.

V2.0.04

2008/03/11

- Correct MOTION_SENSITIVE in MPEG4 and ENCODER CGIs.
- Correct the input argument of VIDEO_SHUTTER_SPEED in ENCODER CGI.
- Add VIDEO_IRIS. VIDEO_BLC_MODE, VIDEO_SENSEUP_LEVEL, VIDEO_DAYNIGHT_MODE, CAMERA_PRESET, DIO_OUTPUT in ENCOER CGI.
- Add the Content-Length in HTTP Header in all POST reply messages (refer to UPDATE and 80503736 CGIs).
- Add PTZ URLs (ADDR, PTZ_VENDOR, ZOOM, ZOOM_POSITION, FOCUS, FOCUS_POSITION, MOVE, MOVE_LIMIT, MOVE_LIMIT_GET, MOVE_MAX_SPEED_GET, POSITION, POSITION_GET) in ENCODER CGI.
- Add PTZ_IMAGE URL in UPDATE CGI.

V2.0.05

2008/05/22

- Add the motion region specification in MOTION_SETTING URL in MPEG4 and MOTION_CONFIG URL in ENCODER.

Description of URL

Specification of Return Message

List by CGI Program

> SYSTEM CGI, MPEG4 CGI, ENCODER CGI, URL CGI, DECODER CGI, UPDATE CGI, QUAD CGI

List by PLATFORM

> WPL Platform
> ENCODER | 1-Channel, 2-Channel, QUAD
> DECODER | 1-Channel
> EPL Platform
> ENCODER | 1-Channel
> DECODER | 1-Channel
> Multi-Channel Encoder
> Router | 4-Channel, 8-Channel, 16-Channel
> Video Server | 4-Channel, 8-Channel, 16-Channel
> Platform T
> ENCODER | 1-Channel, 4-Channel
> DECODER | 1-Channel

Back to

> HOME