AUDIO_LOOP_BACK

Description

> Enable or Disable the Loopback function which routes the AudioIn to AudioOut in firmware side.

> This is for test only and should be used internally.

Input Argument

> 0: Disable, 1: Enable

Attribute

- Write Only
- On-Fly

Return of Message

> AUDIO_LOOP_BACK='0'

Applicability

- EPL Encoder Devices

Status

> Valid

See Also

> NETWORKACCESS_STOP, SET_FRAME_Q_LEN, RS232_TEST

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&AUDIO_LOOP_BACK=0

Back to

> HOME, URL CGI