POSITION

Description

> Move the camera to the specific position.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the error message will be returned.

> MOVE Command | Description
> ABSOLUTE,PositionPan,PositionTilt,SpeedPan,SpeedTilt | Move camera to the specific position with specific speeds. The (PositionPan, PositionTilt) is the distance of position (0,0).
> RELATE,PositionPan,PositionTilt,SpeedPan,SpeedTilt | Move camera to the specific position with specific speeds. The (PositionPan, PositionTilt) is the distance of current camera position.

> The PositionPan and PositionTilt are in hexadeciaml started from 0x0 to 0xFFFF. The PTZ camera might not have such wide range of these positions. However, the device will NOT validate them before parser and handle this URL. Please refer to the device specification to have correct pan and tilt position ranges.

> If the URL does not bring the SpeedTilt and SpeedPan, the current pan and tilt speeds will be used.

> The SpeedPan and SpeedTilt are in hexadecimal and started from 0x1 (slowest) to 0x5 (fastest)

> There are five levels in SpeedPan and SpeedTilt. The PTZ camera might have more levels of them. In case, the linear scaling algorithm will be used for that.

Input Argument

> Refer to above command table

Attribute

- Write Only
- On-Fly

Return of Message

- Write Operation

> OK: echo of command
> or
> ERROR: echo of command

Applicability

- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : 4CH and 16CH Video Servers

Status

> Valid

See Also

> ADDR, PTZ_VENDOR, ZOOM, ZOOM_POSITION, FOCUS_POSITION, MOVE_LIMIT, MOVE_LIMIT_GET, MOVE_MAX_SPEED_GET, POSITION_GET

Example

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&POSITION=ABSOLUTE,0x122,0x333
> or
> http://ip:port/cgi-bin/cmd/encoder?POSITION=ABSOLUTE,0x122,0x333

Back to

> HOME, ENCODER CGI