WAN_ADDRESS

WAN_IP, WAN_NETMASK, WAN_GATEWAY

Description

> Get or Set IP, Netmask or Gateway address of WAN port. These Settings are only valid if only of the WAN_TYPE is Static. If the WAN_TYPE is Dynamic, these settings will be applied if the device fails of getting the address from the DHCP server. The argument of these URL will be checked before apply them. The check mechanism is

> - WAN_IP has to be an unicast IP address.
> - WAN_NETMASK has to be followed the rule of IP Netmask.
> - WAN_GATEWAY has to be an unicast IP address

> Because these URLs are sent separately, the device is not able to check if the WAN_IP and WAN_GATEWAY are in the same subnet.

> In EPL decoder, this URL is same as the WAN_IP, WAN_NETMASK and WAN_GATEWAY in the SYSTEM CGI but only Type1 URL command is supported.

> Therefore, the WAN_IP, WAN_NETMASK and WAN_GATEWAY URLs in WPL decoders are only addressed in this page.

Input Argument

> IPv4 Addressing (xxx.xxx.xxx.xxx)

Attribute

- Write Only
- Not On-Fly

Return of Message

> None

Applicability

- WPL Decoder Devices
- EPL Decoder Devices (refer to WAN_IP, WAN_NETMASK and WAN_GATEWAY in the SYSTEM CGI)

Status

> Valid

See Also

> WAN, WAN_PPPOE_USERNAME, WAN_PPPOE_PASSWORD

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&WAN_IP=192.168.0.100
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&WAN_NETMASK=255.255.255.0
> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&WAN_GATEWAY=192.168.0.254

Back to

> HOME, URL CGI, SYSTEM CGI