TOS

Description

> Get the ToS(Type of Service) configurations. The ToS setting will be set to the ToS field in IP header of every video and audio packet.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the CHANNLE 1 video server's TOS configurations will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> None

Attribute

- Read Only

Return of Message

> VIDEO_TOS_TYPE='1'
> VIDEO_TOS_PRIORITY='Normal-Service'

Applicability

- WPL Platform : All Encoder Devices
- EPL Platform : All Encoder Devices
- PlatfotmT : All Encoder Devices
- Multi-Channel Encoder : All Devices

Status

> Valid but will be obsolete in the future. That will be claimed with the release of device's firmware.

See Also

> VIDEO_TOS_TYPE, VIDEO_TOS_PRIORITY

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&TOS
> or
> http://ip:port/cgi-bin/cmd/system?TOS

Back to

> HOME, SYSTEM CGI