VIDEO_BLC_MODE

VIDEO_DAYNIGHT_MODE

Description

> Get or Set the Light sensor function.

> This URL could force the sensor to work in Day/Night lighting condition or auto-detected by sensor. Please refer the Camera Setup Design Specification for further details.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> DAY, NIGHT or AUTO

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_DAYNIGHT_MODE='AUTO'

- Write Operation

> OK: VIDEO_DAYNIGHT_MODE='AUTO'
> or
> ERROR: VIDEO_DAYNIGHT_MODE='AUTO'

Applicability

- EPL Platform : All Encoders with sensor MT54G15
- PlatfotmT : All Encoders with sensor MT54G15

Status

> Valid

See Also

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_DAYNIGHT_MODE
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_DAYNIGHT_MODE

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_DAYNIGHT_MODE=AUTO
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_DAYNIGHT_MODE=AUTO

Back to

> HOME, ENCODER CGI