CONFIG_GET

Description

> Get the device's configuration.

> The device will reply its configurations as the return message of this URL. Note that some configurations are not the run-time configuration like WAN port configurations.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the router's configuration will be returned. Otherwise, the channel n video server's configuration will be returned.

Input Argument

> None

Attribute

- Read Only

Return of Message

- Read Operation (example)

> WAN_TYPE='1'
> WAN_IP='192.168.0.100'
> WAN_NETMASK='255.255.255.0'
> WAN_GATEWAY='192.168.0.254'
> WAN_PPPOE_USERNAME=''
> WAN_PPPOE_PASSWORD=''
> SPEED_WAN='0'
> LANGUAGE='0'
> PORT_HTTP='80'
> PORT_SEARCH_1='6005'
> PORT_SEARCH_2='6006'
> LAN_HOSTNAME='ACTi'
> DNS_PRIMARY=''
> DNS_SECONDARY=''
> DDNS_TYPE='1'
> DDNS_HOSTNAME=''
> DDNS_SERVICE='dyndns'
> DDNS_USERNAME=''
> DDNS_PASSWORD=''
> DATE_TYPE='2'
> ........

> LAYOUT_FOOTER_COPYRIGHT='Copyright@2003-2008 ACTi Corporation All Right Reserved'
> COMPANY_NAME='ACTi Corporation'
> COMPANY_URL='www.acti.com'
> ACTIVEX_URL=''

Applicability

- WPL Platform : All Encoder Devices
- EPL Platform : All Encoder Devices
- PlatfotmT : All Encoder Devices
- Multi-Channel Encoder : Router Only

Status

> Valid

See Also

> CONFIG_SET, FIRMWARE, FIRMWARE_ALL, PROFILE, PROFILE_PACK

Example

- Write Operation

> http://ip:port/cgi-bin/update?USER=Admin&PWD=123456&CONFIG_GET

Back to

> HOME, UPDATE CGI