URL Command Tester

mpeg4 Video Quality Setting Video Quality Setting 55 Get, Set brightness 55 Get, Set contrast 55 Get, Set Saturation 55 Get, Set Hue Video Setting Video Setting N1280x1024 N1280x720 N720x480 N640x480 N352x240 N176x120 N160x112 P720x576 P640x480 P352x288 P176x144 NTSC to PAL Need SaveReboot 28K 56K 128K 256K 384K 500K 750K 1M 1.2M 1.5M 2M 2.5M 3M Get, Set video bitrate 30 15 10 7 6 5 4 3 2 1 25 12 8 6 5 4 3 2 1 Get, Set video frame number Constant Variable Need SaveReboot Camera Name Camera Name Camera 1 Get, Set camera name Video Status Video Status Get video status DIO DIO DO1 LOW, DO2 LOW DO1 HI , DO2 LOW DO1 LOW, DO2 HI DO1 HI , DO2 HI Set DIO output Get DIO status Motion Detection Motion Detection Disabled Enabled Get, Set motion enabled flag 1,100,100,200,200,70 Set motion detection settings 1,70 Set motion detection sensitivity Get motion detection status Serial Port Serial Port 8N1 8O1 8E1 2400 4800 9600 19200 38400 57600 115200 Get, Set serial port setting Set ASCII data via serial port Set HEX data via serial port RTP Commands RTP Commands PLAY PAUSE Get, Set RTP multicast streaming methods system Device Operation Device Operation Set Save and Reboot command Set Save command Set Reboot command Set Factory Default command Get System Information Get System Parameters Network Setting Network Setting Hostname Get, Set LAN Hostname Get, Set LAN Config Get WAN information Get WAN status Get WAN status v2 Dynamic IP Static IP PPPoE Get, Set WAN Type 192.168.0.100 Get, Set WAN IP Address 255.255.255.0 Get, Set WAN netmask 192.168.0.253 Get, Set WAN gateway username Get, Set PPPoE user name password Get, Set PPPoE password Get DNS information 192.168.1.1 Get, Set primary DNS 192.168.1.2 Get, Set secondary DNS Disabled Enabled Get, Set DDNS type hostname Get, Set DDNS hostname members.dyndns.org members.3322.org www.EZ-IP.Net www.penguinpowered.com members.dhs.org update.ods.org cgi.tzo.com members.easydns.com www.justlinux.com www.dyns.cx www.hn.org www.zoneedit.com Get, Set DDNS service username Get, Set DDNS user name password Get, Set DDNS password Disabled Enabled hostname members.dyndns.org members.3322.org www.EZ-IP.Net www.penguinpowered.com members.dhs.org update.ods.org cgi.tzo.com members.easydns.com www.justlinux.com www.dyns.cx www.hn.org www.zoneedit.com username password Get or Set the DDNS configuration. This is the new added command. All configurations of DDNS will be binded to this command and all settings will be checkes first. This command will replace the DDNS_TYPE, DDNS_HOSTNAME, DDNS_SERVICE, DDNS_USERNAME and DDNS_PASSWORD commands Get the DDNS information Date / Time Setting Date / Time Setting Manual Setting NTP/SNTP Get, Set Date type 192.168.1.35 Get, Set SNTP IP address 5 min 1 Hour 6 Hours 12 Hours 1 Day Get, Set SNTP Update Interval 033100002006 Get, Set Date manually 10:45:58 Get, Set Time manually GMT-12 GMT-11 GMT-10 GMT-09 GMT-08 GMT-07 GMT-06 GMT-05 GMT-04 GMT-03 GMT-02 GMT-01 GMT-00 GMT+01 GMT+02 GMT+03 GMT+04 GMT+05 GMT+06 GMT+07 GMT+08 GMT+09 GMT+10 GMT+11 GMT+12 GMT+13 Get, Set time zone manually Get Date information Type of Service Setting Type of Service Setting Get TOS information Disabled Enabled Get, Set video TOS type Minimize-Delay Maximize-Throughput Maximize-Reliability Minimize-Cost Normal-Service Get, Set TOS Priority Account / Password Account / Password Get Account information Admin Get, Set root account name 123456 Get, Set root account password guest1 Get, Set user1 user name 123456 Get, Set user1 password guest2 Get, Set user2 user name 123456 Get, Set user2 password guest3 Get, Set user3 user name 123456 Get, Set user3 password guest4 Get, Set user4 user name 123456 Get, Set user4 password guest5 Get, Set user5 user name 123456 Get, Set user5 password guest6 Get, Set user6 user name 123456 Get, Set user6 password guest7 Get, Set user7 user name 123456 Get, Set user7 password guest8 Get, Set user8 user name 123456 Get, Set user8 password guest9 Get, Set user9 user name 123456 Get, Set user9 password guest10 Get, Set user10 user name 123456 Get, Set user10 password PORT Setting PORT Setting Get Port information 80 Get, Set HTTP port 6005 Get, Set Search Port 1 6006 Get, Set Search Port 2 6000 Get, Set Register Port 6001 Get, Set Control Port 6002 Get, Set Video Port 5000 Get, Set Multicast Port 7070 Get, Set RTSP Port Language Language 0 - English 1 - Traditional Chinese 2 - Simplified Chinese 3 - Japanese 4 - Spanish 5 - Italian 6 - German 7 - Portuguese 8 - Czech 9 - French Get, Set displayed language Other Other TCP Version 1.0 TCP Version 2.0 Get, Set video streaming type TCP Only for TCP2.0 Multicast Only for TCP2.0 TCP & Multicast for TCP2.0 RTP over UDP for TCP2.0 RTP over Multicast for TCP2.0 RTP over UDP & Multicast for TCP2.0 Get, Set video streaming method Disabled Enabled Get or Set RTSP_AUTHEN. When it is disabled, there is no need to perform the RTSP authentication to get the Video/Audio Stream through RTSP/RTP Disabled Enabled Get or Set B2_RTP_APPENDED. When it is disabled, there is no B2 Frame appended to every RTP video frame LAN Port WAN Port Get, Set multicast interface 228.5.6.1 Get, Set multicast IP address 5000 Get, Set RTP Multicast Video Port 5002 Get, Set RTP Multicast Audio Port Disabled Enabled Get, Set network failover function Disabled Enabled Get, Set IGMP function Auto detect speed 100Mbps/Full Duplex 100Mbps/Half Duplex 10Mbps/Full Duplex 10Mbps/Half Duplex Get, Set LAN speed setting Auto detect speed 100Mbps/Full Duplex 100Mbps/Half Duplex 10Mbps/Full Duplex 10Mbps/Half Duplex Get, Set WAN speed setting 255 Get, Set video multicast TTL 1 Get, Set Multicast IP DISABLE TCP MULTICAST Get, Set LAN port setting DISABLE TCP MULTICAST Get, Set WAN port setting Get the supported video resolutions. It will be permuted to descend to lowest resolution. The ";" will be used to separate the video resolution bwtewwn NTSC and PAL. Get Date information Disable Enable FIRST LAST Mon. Tue. Wed. Thu. Fri. Sat. Sun. Jan. Feb. Mar. Apr. May Jun. Jul. Aug. Sep. Oct. Nov. Dec. FIRST LAST Mon. Tue. Wed. Thu. Fri. Sat. Sun. Jan. Feb. Mar. Apr. May Jun. Jul. Aug. Sep. Oct. Nov. Dec. Get or Set the Datlight saving configuration. Encoder Video Setting Video Setting AUTO INDOOR HOLD_CURRENT ATW MANUAL OUTDOOR Get or Set the VIDEO White Balance Mode configuration. The parameter will be checked first Get or Set the RGain and BGain when White Balance Mode is MANUAL. If the VIDEO_WB_MODE is not MANUAL, this command is not valid. The parameter will be checked first AUTO MANUAL Get or Set the Video Exposure Mode configuration. The parameter will be checked if it is valid Get or Set the Video Exposure Gain when the Video Exposure Mode is Manual. If the VIDEO_EXPOSURE_MODE is not MANAUL, this command is not valid. The parameter will be checked first 25 30 50 60 100 120 250 500 1000 2000 4000 10000 Get or Set the Video Shutter Speed when the Video Exposure Mode is MANUAL. If the VIDEO_EXPOSURE_MODE is not MANUAL, this command is not valid. The reciprocal of parameter gives the shutter speed in sec. For example, the shutter speed is 1/25 sec when the VIDEO_SHUTTER_SPEED=25 AUTO 60HZ 50HZ Get or Set the Video Flickless Mode configuration. The parameter will be checked first MPEG4 MJPEG Get or Set the VIDEO White Balance Mode configuration. The parameter will be checked first 28K 56K 128K 256K 384K 500K 750K 1M 1.2M 1.5M 2M 2.5M 3M Get or Set the Video Bitrate, The change is only effective when the VIDEO_ENCODER=MPEG4 and the VIDEO_MAX_BITRATE=UNLIMITED. The parameter will be checked first 28K 56K 128K 256K 384K 500K 750K 1M 1.2M 1.5M 2M 2.5M 3M UNLIMITED Get or Set the Maximum Video Bitrate, The change is only effective when the VIDEO_ENCODER=MPEG4. This will limited the video bitrate in MPEG4. The parameter will be checked HIGH MIDDLE LOW NONE Get or Set the Video Quality in MPEG4 mode. The change is only effective when the VIDEO_ENCODER=MPEG4. If the parameter is not NONE, the bit rate of the video stream is vary then. To set the parameter to NONE to back to the constant bitr rate mode. Constant Variable Get or Set the Video FPS mode. MODE1=Constant FPS mode. MODE2=Variable FPS Mode. This is the same as the VIDEO_FPS in MPEG4 CGI. The parameter will be checked first Get or Set the constant FPS number in MPEG4 mode. The change is only effective when the VIDEO_ENCODER=MPEG4 and VIDEO_FPS=MODE1. This command is the same as the VIDEO_FPS_NUM in mpeg4 CGI. The parameter will be checked first Get or Set the Variable FPS number in MPEG4 and MJPEG mode. The change is only effective when the VIDEO_FPS=MODE2 and the V2_STREAMING_METHOD=0 or 3. This command is the same as the VIDEO_VARIABLE_FPS in MPEG4 CGI. The parameter will be checked first Get or Set the Video Variable FPS number configuration. This set the number of frames in a second in the variable FPS mode when the host connected the encoder device. The host could change the frame rate by using VIDEO_VARIANLE_FPS command. The setting is only effective when the V2_STREAMING_MODE is not RTP. The parameter will be checked first Get or Set Video Resolution. This is the same as the VIDEO_RESOLUTION in MPEG4 CGI. The parameter will be checked first Get or Set the Video Compression Ratio. The higher value in the parameter get higher video quality and bit rate. The change is only effective when the VIDEO_ENCODER=MJPEG. The parameter will be checked first Get or Set the Video Frame Rate in MJPEG mode. This could limited the encoder to send the number of video frames in a second in MJPEG mode. The change is only effective when the VIDEO_ENCODER=MJPEG and VIDEO_FPS=MODE1. The parameter will be checked first Disable Enable Get or set Motion Enabled configuration. The parameter is in the hexidecimal format. This is the same as the MOTION_ENABLED in MPEG4 CGI. The parameter will be checked first 1 2 3 Read the Motion Configuration if the parameter is NULL. The format of return of command is MOTION_CONFIG=n,sx,sy,ex,ey,sen,time. Set the Motion Configuration to the specific motion region if the parameter is n,sx,sy,ex,ey,sen,time. The motion time give the motion trigger interval which the motion trigger will not be issued if two motion triggers in the motion interval. For Video B2, it will NOT have this limitation 1 2 3 Set the motion sensitivity to the specific motion region. This command is the same as the MOTION_SENSITIVE in MPEG4 CGI 1 2 3 Set the motion timer to the specific motion region. The motion time give the motion trigger interval which the motion trigger will not be issued if two motion triggers in the motion interval. The parameter will be checked first Disable Enable Get or Set the Event Enable Configuration. The parameter will be checked first Get or Set the Motion Pre-trigger time. The unit of this parameter is second. Get or Set the Motion Post-trigger time. The unit of this parameter is second. The motion time give the motion trigger interval which the motion trigger will not be issued if two motion triggers in the motion interval. Get or Set the Event trigger interval. The unit of this parameter is second. Successive events happened in this interval will be treated as one event

MPEG4

Get | Set | Command | Value | Description

SYSTEM

Get | Set | Command | Value | Description

ENCODER

Get | Set | Command | Value | Description