TOS_TYPE

VIDEO_TOS_TYPE

Description

> Get or Set ToS (Type of Service) type configuration. The ToS setting will be set to the ToS field in IP header of every video and audio packet.

> When write, the VIDEO_TOS_TYPE=1 will set the "Normal-Seerver" to the ToS Priority.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNLE 1 video server's TOS configurations will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> 1: Disable
> 2: Enable

Attribute

- Readable and Writable
- On-Fly (except all encoder encoders in WPL Platform)

Return of Message

- Read Operation

> VIDEO_TOS_TYPE='1'

- Write Operation

> OK: VIDEO_TOS_TYPE='1'
> or
> ERROR: VIDEO_TOS_TYPE='1'

Applicability

- WPL Platform : All encoder Devices
- EPL Platform : All encoder Devices
- PlatformT : All encoder Devices
- Multi-Channel Encoder : All Devices

Status

> Valid but will be obsolete in the future. That will be claimed with the release of device's firmware.

See Also

> VIDEO_TOS, VIDEO_TOS_PRIORITY

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&VIDEO_TOS_TYPE
> or
> http://ip:port/cgi-bin/cmd/system?VIDEO_TOS_TYPE

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&VIDEO_TOS_TYPE=1
> or
> http://ip:port/cgi-bin/cmd/system?VIDEO_TOS_TYPE=1

Back to

> HOME, SYSTEM CGI