V2_AUDIO_ENABLED

Description

> Get or Set the device's AudioIn (MIC or Line-IN) configuration. Check the device specification is needed before use this command. If the device does not have audio function, the command is read command and return 0 always.

> If the device supports two-way audio, the AudioOut will not be disabled when the V2_AUDIO_ENABLED=0.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's V2_AUDIO_ENABLED configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> 0 : Disable
> 1 : Enable

Attribute

- Readable and Writable
- On-Fly (except all device in WPL Platform)

Return of Message

- Read Operation

> V2_AUDIO_ENABLED='1'

- Write Operation

> OK: V2_AUDIO_ENABLED='1'
> or
> ERROR: V2_AUDIO_ENABLED='1'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> AUDIO_IN_SENSITIVITY, AUDIO_OUT_VOLUME

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_AUDIO_ENABLED
> or
> http://ip:port/cgi-bin/cmd/system?V2_AUDIO_ENABLED

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_AUDIO_ENABLED=1
> or
> http://ip:port/cgi-bin/cmd/system?V2_AUDIO_ENABLED=1

Back to

> HOME, SYSTEM CGI