DATE_SNTP_UPDATE

DDNS_SNTP_UPDATE

Description

> Get or Set Date update interval in second by SNTP synchronization.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and the Router's DATE configurations will be returned.

Input Argument

> 300, 3600, 21600, 43200, 86400

Attribute

- Readable and Writable (except all video servers in Multi-Channel Platform)
- On-Fly (except all devices in WPL Platform)

Return of Message

- Read Operation

> DATE_SNTP_UPDATE='86400'

- Write Operation

> OK: DATE_SNTP_UPDATE='86400'
> or
> ERROR: DATE_SNTP_UPDATE='86400'

Applicability

- WPL Platform : All Encoder Devices
- EPL Platform : All Encoder Devices
- PlatformT : All Encoder Devices
- Multi-Channel Encoder : All Devices

Status

> This URL will be obsolete and replaced by DATE_CONFIG

See Also

> DATE, DATE_TYPE, DATE_SNTP_IP, DATE_MANUAL_DATE, DATE_MANUAL_TIME, DATE_MANUAL_ZONE, DATE_CONFIG, DAYLIGHT_SAVING_CONFIG

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DATE_SNTP_UPDATE
> or
> http://ip:port/cgi-bin/cmd/system?DATE_SNTP_UPDATE

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DATE_SNTP_UPDATE=86400
> or
> http://ip:port/cgi-bin/cmd/system?DATE_SNTP_UPDATE=86400

Back to

> HOME, SYSTEM CGI