DNS

Description

> Get the DNS (Domain Name Server) configurations.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, the Router's DNS configurations will be returned.

Input Argument

> None

Attribute

- Read Only

Return of Message

> DNS_PRIMARY='168.95.1.1'
> DNS_SECONDARY=''

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> DNS_PRIMARY, DNS_SECONDARY, WAN_STATUS, V2_WAN_STATUS

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&DNS
> or
> http://ip:port/cgi-bin/cmd/system?DNS

Back to

> HOME, SYSTEM CGI