QUAD CGI Program

Only root could set the configuration through this CGI. If the logon user is not root, all write commands will be treated as read commands.

The CGI is only available in the WPL QUAD Encoder Devices.

In QUAD Encoder, it could show 4 channels' video in one single video stream (QUAD Mode) or show one of four channels in one single video stream (Channel Mode).

There is only Type1 URL command supported in this CGI.

The format of the return message does not follow the specification of return message. The return message will be described in every URL command.

List of URLs

> URL | Attribute (R/W, On-Fly)1
> WPL QUAD Encoder
> DISPLAY | RW,V
> OSD_ENABLED | RW,V
> MOTION_ENABLED | RW,V
> SENSITIVE | RW,V
> TITLE_NAME | RW,V
> BRIGHTNESS | RW,V
> CONTRAST | RW,V
> SATURATION | RW,V
> HUE | RW,V

Back to

> HOME

Foot Note

1 | The first part is for Access Mode. It could be RW (Readable and Writeable), RO (Read Only), WO (Write Only) or None (Not Support) The second part is for On-Fly indication. if the change of URL is effective immediately without save and reboot, It could be V (the URL is on-fly). Otherwise, it is X (the URL is not on-fly).