MOTION_ENABLED

Description

> Enable or Disable the Motion Detection function in every channel.

> The input argument of this command is hexadecimal value. It controls how many channels motion detection are enabled or disabled. Here is the map of the input hexadecimal value and the channel motion detection.

> Bit value in the input argument | Channel Motion Detection
> Bit 0 | Channel 1 Motion Detection Function
> Bit 1 | Channel 2 Motion Detection Function
> Bit 2 | Channel 3 Motion Detection Function
> Bit 3 | Channel 4 Motion Detection Function

> The bit value is 1, the corresponding channel motion detection is enabled. Otherwise, it is disable.

Input Argument

> 0xnn

> Note that the value in higher bit (bit 4~7) will not be acceptable and error message will be returned if the higher bit (but 5~7) is not zero.

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> MOTION_ENABLED='0x00'

- Write Operation

> MOTION_ENABLED='0x00'
> or
> ERROR: MOTION_ENABLED Value Failed

Applicability

- WPL Platform : QUAD Encoder Only

Status

> Valid

See Also

> SENSITIVE

Example

- Read Operation

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&MOTION_ENABLED

- Write Operation

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&MOTION_ENABLED=0x00

Back to

> HOME, QUAD CGI