WAN_PPPOE

WAN_PPPOE_USERNAME, WAN_PPPOE_PASSWORD

Description

> Get or set the PPPoE configuration on WAN port. These Settings are only valid if only if the WAN_TYPE is PPPoE. The input argument string length will be checked before apply it.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL will be treated as read-only command and the Router's WAN port PPPoE setting will be returned.

Input Argument

> Character strings (< 64 Bytes)

Attribute

- Readable and Writable (except video server in Multi-Channel Platform)
- Not On-Fly

Return of Message

- Read Operation

> WAN_PPPOE_USERNAME=''
> WAN_PPPOE_PASSWORD=''

- Write Operation

> OK: WAN_PPPOE_USERNAME=''
> OK: WAN_PPPOE_PASSWORD=''
> or
> ERROR: WAN_PPPOE_USERNAME=''
> ERROR: WAN_PPPOE_PASSWORD=''

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> WAN, WAN_STATUS, V2_WAN_STATUS, WAN_TYPE, WAN_IP, WAN_NETMASK, WAN_GATEWAY

Example

- Read Opeation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&WAN_PPPOE_USERAME
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&WAN_PPPOE_PASSWORD
> or
> http://ip:port/cgi-bin/cmd/system?WAN_PPPOE_USERNAME
> http://ip:port/cgi-bin/cmd/system?WAN_PPPOE_PASSWORD

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&WAN_PPPOE_USERAME=''
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&WAN_PPPOE_PASSWORD=''
> or
> http://ip:port/cgi-bin/cmd/system?WAN_PPPOE_USERNAME=''
> http://ip:port/cgi-bin/cmd/system?WAN_PPPOE_PASSWORD=''

Back to

> HOME, SYSTEM CGI

¡@