SET_FRAME_Q_LEN

Description

> Set the maximum of the video frame queue length.

> This is for test only and should be used internally.

Input Argument

> 1~4

Attribute

- Write Only
- On-Fly

Return of Message

> SET_FRAME_Q_LEN='3'

Applicability

- EPL Encoder Devices

Status

> Valid

See Also

> NETWORKACCESS_STOP, RS232_TEST, AUDIO_LOOP_BACK

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&SET_FRAME_Q_LEN=3

Back to

> HOME, URL CGI