VIDEO_WB_MODE

Description

> Get or Set the VIDEO White Balance Mode configuration.

> The availability of white balance and the mode in the video white balance depend on the capability of the sensor in the sensor. For video server, this feature is not available. In some camera sensors, the white balance and the video exposure have very strong link. Then video exposure might be adapted automatically as the white balance was changed. Please refer the Camera Setup Design Specification for further details.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> AUTO, INDOOR1, INDOOR2, OUTDOOR1, OUTDOOR2, HOLD, MANUAL

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_WB_MODE='AUTO'

- Write Operation

> OK: VIDEO_WB_MODE='AUTO'
> or
> ERROR: VIDEO_WB_MODE='AUTO'

Applicability

- EPL Platform : All Encoders with sensor MT9V135 or MT9M131
- PlatfotmT : All Encoders with sensor MT9M131

Status

> Valid

See Also

> VIDEO_WB_GAIN, VIDEO_EXPOSURE_MODE, VIDEO_EXPOSURE_GAIN, VIDEO_AGC_GAIN, VIDEO_SHUTTER_MODE, VIDEO_SUHTTER_SPEED,VIDEO_MAX_SHUTTER, VIDEO_FLICKLESS

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_WB_MODE
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_WB_MODE

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_WB_MODE=AUTO
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_WB_MODE=AUTO

Back to

> HOME, ENCODER CGI