PORT_RTP

V2_PORT_RTSP, V2_PORT_RTP_MULTI_VIDEO, V2_PORT_RTP_MULTI_AUDIO

Description

> Get or Set device's RTSP server port number and the multicast port numbers for multicast video and audio RTP streams. When write, the port number will be checked if it was used from other applications. The video and audio RTP ports have to be even ports.

> V2_PORT_RTSP

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this will set the part base of all channels. The RTSP port of the CHANNEL n will be the RTSP port base + 2 * (n -1). For example, the V2_PORT_RTSP=7070 will set the base of RTSP port to 7070. Then, the RTSP port of CHANNEL 1 is 7070, the control port of CHANNEL 2 is 7072.

> V2_PORT_RTP_MULTI_VIDEO, V2_PORT_RTP_MULTI_AUDIO

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this will set the port base of all channels. The multicast port of all CHANNELs will be this multicast port. For example, the V2_PORT_RTP_MULTI_VIDEO=5000 and V2_PORT_RTP_MULTI_AUDIO=5002 will set the RTP multicast port of all CHANNEL to 5000 for video and 5002 for audio.

Input Argument

> URL Commnd Name | Description
> V2_PORT_RTSP | TCP port number, 1~65535
> V2_PORT_RTP_MULTI_VIDEO | even UDP port number, 2~65534
> V2_PORT_RTP_MULTI_AUDIO | even UDP port number, 2~65534

Attribute

- Readable and Writable
- On-Fly (except all encoder in WPL Platforms)

Return of Message

- Read Operation

> V2_PORT_RTSP='7007'
> V2_PORT_RTP_MULTI_VIDEO='5000'
> V2_PORT_RTP_MULTI_AUDIO='5002'

- Write Operation

> OK: V2_PORT_RTSP='7007'
> OK: V2_PORT_RTP_MULTI_VIDEO='5000'
> OK: V2_PORT_RTP_MULTI_AUDIO='5002'
> or
> ERROR: V2_PORT_RTSP='7007'
> ERROR: V2_PORT_RTP_MULTI_VIDEO='5000'
> ERROR: V2_PORT_RTP_MULTI_AUDIO='5002'

Applicability

- WPL Platform : All Encoder Devices
- EPL Platform : All Encoder Devices
- PlatformT : All Encoder Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> PORT, PORT_HTTP, PORT_SEARCH_1, PORT_SEARCH_2, PORT_SEARCH, PORT_REGISTER, PORT_CONTROL, PORT_VIDEO, PORT_MULTICAST

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_PORT_RTSP
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_PORT_RTP_MULTI_VIDEO
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_PORT_RTP_MULTI_AUDIO
> or
> http://ip:port/cgi-bin/cmd/system?V2_PORT_RTSP
> http://ip:port/cgi-bin/cmd/system?V2_PORT_RTP_MULTI_VIDEO
> http://ip:port/cgi-bin/cmd/system?V2_PORT_RTP_MULTI_AUDIO

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_PORT_RTSP=7070
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_PORT_RTP_MULTI_VIDEO=5000
> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_PORT_RTP_MULTI_AUDIO=5002
> or
> http://ip:port/cgi-bin/cmd/system?V2_PORT_RTSP=7070
> http://ip:port/cgi-bin/cmd/system?V2_PORT_RTP_MULTI_VIDEO=5001
> http://ip:port/cgi-bin/cmd/system?V2_PORT_RTP_MULTI_AUDIO=5002

Back to

> HOME, SYSTEM CGI