VIDEO_ADJUST

VIDEO_BRIGHTNESS, VIDEO_CONTRAST, VIDEO_SATURATION, VIDEO_HUE

Description

> Get or set the video parameters.

> Note that VIDEO_HUE is Read-Only in some EPL and PlatformT encoders. Please check devices' specifications.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's VIDEO_BRIGHTNESS configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> 0~100.

Attribute

- Readable and Writable
- On-Fly

Return of Message

-     Read Operation

> OK: VIDEO_BRIGHTNESS='50'
> OK: VIDEO_CONTRAST='50'
> OK: VIDEO_SATURATION='50'
> OK: VIDEO_HUE='50'

- Write Operation

> OK: VIDEO_BRIGHTNESS='50'
> OK: VIDEO_CONTRAST='50'
> OK: VIDEO_SATURATION='50'
> OK: VIDEO_HUE='50'
> or
> ERROR: VIDEO_BRIGHTNESS='50'
> ERROR: VIDEO_CONTRAST='50'
> ERROR: VIDEO_SATURATION='50'
> ERROR: VIDEO_HUE='50'

Applicability

- WPL Platform : All 1CH and 2CH Encoders
- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : All Video Servers

Status

> Valid

See Also

> ¡@

Example

- Read Operation

> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_BRIGHTNESS
> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_CONTRAST
> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_SATURATION
> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_HUE
> or
> http://ip:port/cgi-bin/cmd/mpeg4? VIDEO_BRIGHTNESS
> http://ip:port/cgi-bin/cmd/mpeg4? VIDEO_CONTRAST
> http://ip:port/cgi-bin/cmd/mpeg4? VIDEO_SATURATION
> http://ip:port/cgi-bin/cmd/mpeg4? VIDEO_HUE

- Write Operation

> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_BRIGHTNESS=50
> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_BRIGHTNESS=50
> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_BRIGHTNESS=50
> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&VIDEO_BRIGHTNESS=50
> or
> http://ip:port/cgi-bin/cmd/mpeg4? VIDEO_BRIGHTNESS=50
> http://ip:port/cgi-bin/cmd/mpeg4? VIDEO_BRIGHTNESS=50
> http://ip:port/cgi-bin/cmd/mpeg4? VIDEO_BRIGHTNESS=50
> http://ip:port/cgi-bin/cmd/mpeg4? VIDEO_BRIGHTNESS=50

Back to

> HOME, MPEG4 CGI