PORT_HTTP

Description

> Get or Set device's http server port number. When write, the port number will be checked if it was used from other applications.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, this URL is read-only command and the Router's http server port number will be returned.

Input Argument

> TCP port number, 1~65535

Attribute

- Readable and Writable (except all video servers in Multi-Channel Encoder)
- Not On-Fly

Return of Message

- Read Operation

> PORT_HTTP='80'

- Write Operation

> OK: PORT_HTTP='80'
> or
> ERROR: PORT_HTTP='80'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> PORT, PORT_SEARCH_1, PORT_SEARCH_2, PORT_SEARCH, PORT_REGISTER, PORT_CONTROL, PORT_VIDEO, PORT_MULTICAST, V2_PORT_RTSP, V2_PORT_RTP_MULTI_VIDEO, V2_PORT_RTP_MULTI_AUDIO

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&PORT_HTTP
> or
> http://ip:port/cgi-bin/cmd/system?PORT_HTTP

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&PORT_HTTP=80
> or
> http://ip:port/cgi-bin/cmd/system?PORT_HTTP=80

Back to

> HOME, SYSTEM CGI