VIDEOSERVER

Description

> Get the settings of encoder which the device connects to. The setting include

> CHxx_VIDEO_CONNECT, CHxx_VIDEO_STREAM, CHxx_VIDEO_AUDIO, CHxx_VIDEO_CONTROL, CHxx_VIDEO_TCP_IP, CHxx_VIDEO_MULTICAST_IP, CHxx_VIDEO_USERNAME, CHxx_VIDEO_PASSWORD, CHxx_TIME, CHxx_PORT_STREAMIN, CHxx_PORT_CONTROL, CHxx_PORT_MULTICAST, CHxx_PORT_RTP and CHxx_PORT_HTTP

> where xx is the channel number of the connected encoder. The channel number is started from 01.

Input Argument

> None

Attribute

- Read Only

Return of Message

> CHxx_VIDEO_CONNECT='1'
> CHxx_VIDEO_STREAM='1'
> CHxx_VIDEO_AUDIO='0'
> CHxx_VIDEO_CONTROL='1'
> CHxx_VIDEO_TCP_IP='172.16.3.59'
> CHxx_VIDEO_MULTICAST_IP='228.5.6.1'
> CHxx_VIDEO_USERNAME='Admin'
> CHxx_VIDEO_PASSWORD='123456'
> CHxx_TIME='0'
> CHxx_PORT_STREAMIN='6002'
> CHxx_PORT_CONTROL='6001'
> CHxx_PORT_MULTICAST='5000'
> CHxx_PORT_RTP='7070'
> CHxx_PORT_HTTP='80'

> where xx is the channel number started from 01.

Applicability

- WPL Decoder Devices

Status

> Valid

See Also

> ¡@

Example

- Read Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&VIDEOSERVER

Back to

> HOME, URL CGI