OSD_POSITION_RANGE

OSD

Description

> Get the OSD configurations.

Input Argument

> None

Attribute

- Read Only

Return of Message

- Read Operation

> OSD_FORMAT='0x2f'
> OSD_POSITION_RANGE='1,100,1,100'
> OSD_POSITION='10,10'
> OSD_DATE_FORMAT='1'

Applicability

- WPL Decoder Devices
- EPL Decoder Devices
- PlatformT Decoder Devices

Status

> Valid

See Also

> OSD_FORMAT, OSD_POSITION, OSD_POSITION_RANGE, OSD_DATE_FORMAT

Example

- Read Operation

> http://ip:port/cgi-bin/decoder?USER=Admin&PWD=123456&OSD
> or
> http://ip:port/cgi-bin/cmd/decoder?OSD

Back to

> HOME, DECODER CGI