VIDEO_SHUTTER_MODE

Description

> Get or Set the VIDEO Shutter Mode configuration.

> Some sensors, like MT9V135 and MT9M131, the video shutter mode is associated with the video exposure mode. Please refer the Camera Setup Design Specification for further details. Therefore, this URL is not valid in the encoder which its sensor is MT9V135 and MT9M131.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> AUTO, MANUAL

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_SHUTTER_MODE='AUTO'

- Write Operation

> OK:VIDEO_SHUTTER_MODE='AUTO'
> or
> ERROR: VIDEO_SHUTTER_MODE='AUTO'

Applicability

> None

Status

> Valid

See Also

> VIDEO_WB_MODE, VIDEO_WB_GAIN, VIDEO_EXPOSURE_GAIN, VIDEO_AGC_GAIN, VIDEO_SUHTTER_SPEED,VIDEO_MAX_SHUTTER, VIDEO_FLICKLESS

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_SHUTTER_MODE
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_SHUTTER_MODE

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_SHUTTER_MODE=AUTO
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_SHUTTER_MODE=AUTO

Back to

> HOME, ENCODER CGI