DISPLAY

Description

> Get or Set video display mode configuration.

> The device is in the QUAD mode if The input argument is 0. Otherwise, the device is in the Channel Mode.

Input Argument

> n
> where
> n : 0: Display 4 Channels' video in one single video stream. (QUAD Mode)
> 1: Display Channel 1 video in one single video stream (Channel Mode)
> 2: Display Channel 2 video in one single video stream (Channel Mode)
> 3: Display Channel 3 video in one single video stream (Channel Mode)
> 4: Display Channel 4 video in one single video stream (Channel Mode)

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> DISPLAY='0'

- Write Operation

> DISPLAY='0'
> or
> ERROR: DISPLAY Value Failed

Applicability

- WPL Platform : QUAD Encoder Only

Status

> Valid

See Also

¡@

Example

- Read Operation

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&DISPLAY

- Write Operation

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&DISPLAY=0

Back to

> HOME, QUAD CGI