OSD_POSITION

OSD_FORMAT

Description

> Get or Set the OSD format on the TV screen.

> The Decoder could show some information of Encoder or itself on the TV screen. The value in some bits in input argument of this URL controls if the specific information could be on the TV screen or not. The bitmap of the input argument and the OSD information is listed below.

> bit in the Input argument | Information on the OSD
> BIT 0 | Date and Time information of the encoder
> BIT 1 | The IP addresses of the encoder
> BIT 2 | The camera name of the encoder
> BIT 3 | The IP addresses of the Decoder
> BIT 4 | The Motion Trigger form the encoder
> BIT 5 | The DI Trigger from the Decoder

> When the bit in the input argument is set, the associated information will be shown on the OSD. Otherwise, the associated information will not be shown. For example, the Date and Camera name will be shown on the OSD in the OSD_FORMAT=0x05.

> The high bits, bit 6 and 7, in the input argument value will be ignored if they are not zero.

Input Argument

> Hexadecimal Value: 0x00~0x2F.

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OSD_FORMAT='0x2f'

- Write Operation

> OK: OSD_FORMAT='0x2f'
> or
> ERROR: OSD_FORMAT='0x2f'

Applicability

- WPL Decoder Devices
- EPL Decoder Devices
- PlatformT Decoder Devices

Status

> Valid

See Also

> OSD, OSD_POSITION, OSD_POSITION_RANGE, OSD_DATE_FORMAT

Example

- Read Operation

> http://ip:port/cgi-bin/decoder?USER=Admin&PWD=123456&OSD_FORMAT
> or
> http://ip:port/cgi-bin/cmd/decoder?OSD_FORMAT

- Write Operation

> http://ip:port/cgi-bin/decoder?USER=Admin&PWD=123456&OSD_FORMAT=0x2f
> or
> http://ip:port/cgi-bin/cmd/decoder?OSD_FORMAT=0x2f

Back to

> HOME, DECODER CGI