VIDEO_ENCODER

Description

> Get or Set the type of the encoding engine in encoder.

> Note that some video configurations, like VIDEO_BITRATE, will be changed when the VIDEO_ENCODER was changed.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's MOTION_ENABLED configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> MJPEG, MPEG4, H264

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_ENCODER='MPEG4'

- Write Operation

> OK: VIDEO_ENCODER='MPEG4'
> or
> ERROR: VIDEO_ENCODER='MPEG4'

Applicability

- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : 4CH and 16CH Video Servers

Status

> Valid

See Also

- In mpeg4 CGI

> VIDEO_BITRATE

- In encoder CGI

> VIDEO_BITRATE, VIDEO_MAX_BITRATE, VIDEO_MPEG4_QUALITY, VIDEO_H264_QUALITY, VIDEO_FPS_NUM, VIDEO_H264_FPS, VIDEO_MJPEG_FPS

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_ENCODER
> or
> http://ip:port/cgi-bin/cmd/encoder?VIDEO_ENCODER

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_ENCODER=MPEG4
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_ENCODER=MPEG4

Back to

> HOME, MPEG4 CGI, ENCODER CGI