MOTION_STATUS

Description

> Get the Motion settings.

> This URL could read the basic motion configurations from device. The basic motion configuration includes the motion region ID, location of the motion region (rectangular area) and the sensitivity of the motion region. For getting complete motion configurations, the URL MOTION_CONFIG in encoder CGI is used.

> The format of the return message in this URL is
> n,ex,ey,sx,sy,sen
> where
> n is the motion region started from 1,
> (ex,ey) is the coordinate in pixel of the left-top corner of the motion region.
> (sx,sy) is the coordinate in pixel of the right-button corner of the motion region
> sen is the sensitivity of the motion region and the range is 0~100.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's MOTION_STATUS configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> None

Attribute

- Read only

Return of Message

-     Read Operation

>     MOTION_STATUS=1,0,0,0,0,0
>     MOTION_STATUS=2,0,0,0,0,0
>     MOTION_STATUS=3,0,0,0,0,0

Applicability

- WPL Platform : All Encoders
- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : All Video Servers

Status

> Valid

See Also

- In mpeg4 CGI

> MOTION_ENABLED, MOTION_SETTING, MOTION_SENSITIVITY

- In encoder CGI

> MOTION_ENABLED, MOTION_CONFIG, MOTION_CONFIG_GET, MOTION_SENSITIVITY, MOTION_TIMER, MOTION_OBJ

Example

- Read Operation

> http://ip:port/cgi-bin/mpeg4?USER=Admin&PWD=123456&MOTION_STATUS
> or
> http://ip:port/cgi-bin/cmd/mpeg4?MOTION_STATUS

Back to

> HOME, MPEG4 CGI, ENCODER CGI