RTSP_AUTHEN

Description

> Get or Set the RTSP Authentication function. For security consideration, there needs the RTSP authentication during the RTSP signalling between the encoder and remote device before the RTP video/audio streaming. However, some applications are not much security concerned, it allows to get the RTP video/audio streams without RTSP authentication. Then, this function is disabled. By default, this function is enabled.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNLE 1 video server's RTSP_AUTHEN configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> 1: Disable
> 2: Enable

Attribute

- Readable and Writable (except router in Multi-Channel Platform)
- On-Fly (except all encoders in WPL Platform)

Return of Message

- Read Operation

> RTSP_AUTHEN='2'

- Write Operation

> OK: RTSP_AUTHEN='2'
> or
> ERROR: RTSP_AUTHEN='2'

Applicability

- WPL Platform : All 1CH Encoder Devices (Version after V2.06.12)
- EPL Platform : All encoder Devices (Version after V3.06.03)
- PlatformT : All encoder Devices (Version after V4.00.00)
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> RTP_B2

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&RTSP_AUTHEN
> or
> http://ip:port/cgi-bin/cmd/system?RTSP_AUTHEN

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&RTSP_AUTHEN=2
> or
> http://ip:port/cgi-bin/cmd/system?RTSP_AUTHEN=2

Back to

> HOME, SYSTEM CGI