VIDEO_H264_FPS

Description

> Get or set the FPS (Frame Per Second) number (Frame Rate) configuration in the VIDEO_FPS is MODE1 when the VIDEO_ENCODER is H264

> This URL will not take effect if the VIDEO_FPS is MODE2.

> The supported constant FPS number depends on the sensor and encoder (platform) capabilities. Here is the summary of the FPS number with sensors and encoders. Note that supported constant FPS number listed blow doesn't mean you could set them successfully. You need to check the return code to see if the URL was set successfully.

> - PlatformT

>   Encoder Type | TV Standard | Supported FPS Number
>   Camera (sensor is MT9M131) | NTSC @ N1280x1024 | ¡@
>   NTSC @ N1280x720 | ¡@
>   NTSC @ N640x480 | ¡@
>   Video Server | NTSC (auto sense, not configurable) | 1,2,3,4,5,6,7,10,15,30
>   ¡@ | PAL (auto sense, not configurable) | 1,2,3,4,5,6,8,12,25

Input Argument

> FPS Number. Refer to the table above

Attribute

- Readable and Writable
- On-Fly

Return of Message

-     Read Operation

> OK: VIDEO_H264_FPS='30'

- Write Operation

> OK: VIDEO_H264_FPS='30'
> or
> ERROR: VIDEO_H264_FPS='30'

Applicability

- PlatfotmT : All Encoders

Status

> Valid

See Also

- In mpeg4 CGI

> VIDEO_FPS, VIDEO_VARIABLE_FPS

- In encoder CGI

> VIDEO_FPS, VIDEO_VARIABLE_FPS, VARIABLE_FPS_NUM, VIDEO_FPS_NUM, VIDEO_MJPEG_FPS

- In system CGI

> VIDEO_FPS (Read-Only)

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_H264_FPS
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_H264_FPS

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_H264_FPS=30
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_H264_FPS=30

Back to

> HOME, MPEG4 CGI, ENCODER CGI