VIDEO_WB_GAIN

Description

> Get or Set the R-Gain and B-Gain.

> The video R-Gain and B-Gain is only configurable if only of the VIDEO_WB_MODE is MANUAL. Please refer the Camera Setup Design Specification for further details.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> n,m
> where
> n : 1~100 for R-Gain value
> m : 1~100 for B-Gain value

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_WB_GAIN='128,128'

- Write Operation

> OK: VIDEO_WB_GAIN='128,128'
> or
> ERROR: VIDEO_WB_GAIN='128,128'

Applicability

- EPL Platform : All Encoders with sensor MT9V135 or MT9M131
- PlatfotmT : All Encoders with sensor MT9M131

Status

> Valid

See Also

> VIDEO_WB_MODE, VIDEO_EXPOSURE_MODE, VIDEO_EXPOSURE_GAIN, VIDEO_AGC_GAIN, VIDEO_SHUTTER_MODE, VIDEO_SUHTTER_SPEED,VIDEO_MAX_SHUTTER, VIDEO_FLICKLESS

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_WB_GAIN
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_WB_GAIN

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_WB_GAIN=128,128
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_WB_GAIN=128,128

Back to

> HOME, ENCODER CGI