V2_STREAMING_METHOD

Description

> Get or Set the method of video/audio streaming on the encoder.

> There are numbers of streaming methods the encoder to stream the video and audio data. These method might vary among different devices in different platform.

> In WPL, EPL and Multi-Channel Encoders, only one method is allowed to be available. That means the streaming connection between encoder and remote host will be closed if the streaming method is changed.

> In PlatformT Encoders, all streaming methods could exist at the same time.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's V2_STREAMING_METHOD configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

> Here is the list of the available streaming method vs encoder in different platforms.

> Encoder Type | Supported Streaming Method
> Encoder in WPL Platform | TCP Only
> Multicast Over UDP
> TCP and Multicast
> RTP Over UDP
> RTP Over Multicast
> RTP Over UDP and Multicast
> Encoder in EPL Platform | TCP Only
> Multicast Over UDP
> RTP Over UDP
> RTP Over Multicast
> RTP Over UDP and Multicast
> Encoder In Multi-Channel Platform | TCP Only
> Multicast Over UDP
> TCP and Multicast (8CH Only)
> RTP Over UDP
> RTP Over Multicast
> RTP Over UDP and Multicast
> Encoder in PlatformT Platform | TCP Only
> Multicast Over UDP
> TCP and Multicast (8CH Only)
> RTP Over UDP
> RTP Over Multicast
> RTP Over UDP and Multicast

Input Argument

> 0 : TCP Only
> 1 : Multicast Over UDP
> 2 : TCP and Multicast
> 3. RTP Over UDP
> 4. RTP Over Multicast
> 5: RTP Over UDP and Multicast

Attribute

- Readable and Writable (except routers in Multi-Channel Platform)
- On-Fly (except all encoders in WPL Platform)

Return of Message

- Read Operation

> V2_STREAMING_METHOD='0'

- Write Operation

> OK: V2_STREAMING_METHOD='0'
> or
> ERROR: V2_STREAMING_METHOD='0'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatformT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> V2_STREAMING_TYPE, PROTOCOL_TYPE

Example

- Read Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_STREAMING_METHOD
> or
> http://ip:port/cgi-bin/cmd/system?V2_STREAMING_METHOD

- Write Operation

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_STREAMING_METHOD=0
> or
> http://ip:port/cgi-bin/cmd/system?V2_STREAMING_METHOD=0

Back to

> HOME, SYSTEM CGI