VIDEO_FLICKLESS

Description

> Get or Set the video flickless mode.

> The change of the video flickless will change the base frequency of the shutter speed. For example, the flickless was changed from 60Hz to 50Hz, the shutter speed base will be changed from 1/30,1/60,1/120 to 1/25, 1/50, 1/100 seconds. Then the light condition in the sensor was changed too. Please refer the Camera Setup Design Specification for further details.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> 50HZ, 60HZ

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_FLICKLESS='60HZ'

- Write Operation

> OK: VIDEO_FLICKLESS='60HZ'
> or
> ERROR: VIDEO_FLICKLESS='60HZ'

Applicability

- EPL Platform : All Encoders with sensor MT9V135 or MT9M131
- PlatfotmT : All Encoders with sensor MT9M131

Status

> Valid

See Also

> VIDEO_WB_MODE, VIDEO_WB_GAIN, VIDEO_EXPOSURE_MODE, VIDEO_EXPOSURE_GAIN, VIDEO_AGC_GAIN, VIDEO_SHUTTER_MODE, VIDEO_SUHTTER_SPEED,VIDEO_MAX_SHUTTER,

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_FLICKLESS
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_FLICKLESS

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_FLICKLESS=60HZ
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_FLICKLESS=60HZ

Back to

> HOME, ENCODER CGI