WAN_STATUS

Description

> Get the WAN port runtime status. The device will try to PING the Gateway to know if the WAN connection is alive and www.hinet.net to know if the DNS settings are working. The DDNS status will be returned as well.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, the Router's runtime status will be returned.

Input Argument

> None

Attribute

- Read Only
- Not On-Fly

Return of Message

> WAN_IP='192.168.0.100'
> WAN_NETMASK='255.255.255.0'
> WAN_GATEWAY='192.168.0.254'
> DNS Statue : Connected
> DDNS Status: Connected

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> WAN, V2_WAN_STATUS, WAN_TYPE, WAN_IP, WAN_NETMASK, WAN_GATEWAY, WAN_PPPOE_USERNAME, WAN_PPPOE_PASSWORD

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&WAN_STATUS
> or
> http://ip:port/cgi-bin/cmd/system?WAN_STATUS

Back to

> HOME, SYSTEM CGI