VIDEO_MIRROR_MODE

Description

> Mirror control of the video image.

> When set (=1), the video image will be mirrored.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> 0: Not Mirror, 1: Mirror the image

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_MIRROR_MODE='0'

- Write Operation

> OK:VIDEO_MIRROR_MODE='0'
> or
> ERROR: VIDEO_MIRROR_MODE='0'

Applicability

- EPL Platform : All Encoders with sensor MT9V135 or MT9M131
- PlatfotmT : All Encoders with sensor MT9M131

Status

> Valid

See Also

> VIDEO_FLIP_MODE, LENS_COMPENSATION, DAY_GAIN_THD

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_MIRROR_MODE
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_MIRROR_MODE

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_MIRROR_MODE=0
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_MIRROR_MODE=0

Back to

> HOME, ENCODER CGI