NETWORKACCESS_STOP

Description

> Stop the networking thread in the decoder and show the color bar on the TV Out.

> This is for test only and should be used internally.

Input Argument

> None

Attribute

- Write Only
- On-Fly

Return of Message

> NETWORKACCESS_STOP

Applicability

- EPL Encoder Devices

Status

> Valid

See Also

> SET_FRAME_Q_LEN, RS232_TEST, AUDIO_LOOP_BACK

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&NETWORKACCESS_STOP

Back to

> HOME, URL CGI