VIDEO_OSD

Description

> Enable or Disable to show the specific information of the encoder or decoder on the OSD.

> The Decoder could show some information of Encoder or itself on the TV screen. The information is listed below.

> Information on the OSD | Related URL
> Date and Time information of the encoder | OSD_DATE_TIME, OSD_DATE_FORMAT
> The IP addresses of the encoder | OSD_SERVER_IP
> The camera name of the encoder | OSD_CAMERA_NAME
> The IP addresses of the Decoder | OSD_LOCAL_IP
> The Motion Trigger form the encoder | OSD_MOTION_DETECT
> The DI Trigger from the Decoder | OSD_STATUS

> The value in some bits in input argument of this URL controls if the specific information could be on the TV screen or not. The bitmap of the input argument and the OSD information is listed below.

> bit in the Input argument | Information on the OSD
> BIT 0 | Date and Time information of the encoder
> BIT 1 | The IP addresses of the encoder
> BIT 2 | The camera name of the encoder
> BIT 3 | The IP addresses of the Decoder
> BIT 4 | The Motion Trigger form the encoder
> BIT 5 | The DI Trigger from the Decoder

> When the bit in the input argument is set, the associated information will be shown on the OSD. Otherwise, the associated information will not be shown. For example, the Date and Camera name will be shown on the OSD in the VIDEO_OSD=0x05.

Input Argument

> Hexadecimal Value: 0x00~0x2F.

Attribute

- Write Only
- On-Fly

Return of Message

> None

Applicability

- WPL Decoder Devices

Status

> Valid

See Also

> HOST(only available in WPL Decoder Devices), OSD_X, OSD_Y

Example

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&VIDEO_OSD=0x2f

Back to

> HOME, URL CGI