CHxx_SOURCE_TYPE

Description

> Get or Set the what kind of encoder in this channel the decoder connects to.

> There are three types of encoders, 1CH encoder, Quad Channel Encoder and Multi-Channel Encoder.

> The mapping of the input argument and the type of encoder is listed below.

> Input Argument | Type of Encoder
> 0 | 1CH Encoder
> 1 | QUAD Channel Encoder
> 2 | Multi-Channel Encoder

> The xx is the channel ID in the decoder started from 01 and ended to 16.

> In EPL decoder device, the xx is fixed to 01.

Input Argument

> 0, 1 or 2

Attribute

- Readable and Writable in EPL Decoders
- Not On-Fly

Return of Message

- Read Operation

> CHxx_SOURCE_TYPE='1'

- Write Operation

> OK: CHxx_SOURCE_TYPE='1'
> or
> ERROR: CHxx_SOURCE_TYPE='1'

Applicability

- EPL Decoder Devices

Status

> Valid

See Also

> CHxx_VIDEO_CONNECT, CHxx_VIDEO_VARFPS, CHxx_VIDEO_STREAM, CHxx_VIDEO_AUDIO, CHxx_VIDEO_CONTROL, CHxx_VIDEO_TCP_IP, CHxx_VIDEO_MULTICAST_IP, CHxx_VIDEO_USERNAME, CHxx_VIDEO_PASSWORD, CHxx_PORT_STREAM, CHxx_PORT_CONTROL, CHxx_PORT_MULTICAST, CHxx_PORT_RTP, CHxx_PORT_HTTP, CHxx_TIME, CHxx_QUAD_CHANNEL, CHxx_CHANNEL, SWITCH, VIDEO_VARFPS

Example

- Read Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CHxx_SOURCE_TYPE
> where xx is from 01~16

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&CHxx_SOURCE_TYPE=1
> where xx is from 01~16

Back to

> HOME, URL CGI