VIDEO_EXPOSURE_MODE

Description

> Get or Set the VIDEO Exposure Mode configuration.

> Some sensors, like MT9V135 and MT9M131, the video exposure mode is associated with the video white balance mode. Please refer the Camera Setup Design Specification for further details.

> The error message will be returned if the encoder does not support this URL.

Input Argument

> AUTO, MANUAL

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: VIDEO_EXPOSURE_MODE='AUTO'

- Write Operation

> OK: VIDEO_EXPOSURE_MODE='AUTO'
> or
> ERROR: VIDEO_EXPOSURE_MODE='AUTO'

Applicability

- EPL Platform : All Encoders with sensor MT9V135 or MT9M131
- PlatfotmT : All Encoders with sensor MT9M131

Status

> Valid

See Also

> VIDEO_WB_MODE, VIDEO_WB_GAIN, VIDEO_EXPOSURE_GAIN, VIDEO_AGC_GAIN, VIDEO_SHUTTER_MODE, VIDEO_SUHTTER_SPEED,VIDEO_MAX_SHUTTER, VIDEO_FLICKLESS

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_EXPOSURE_MODE
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_EXPOSURE_MODE

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&VIDEO_EXPOSURE_MODE=AUTO
> or
> http://ip:port/cgi-bin/cmd/encoder? VIDEO_EXPOSURE_MODE=AUTO

Back to

> HOME, ENCODER CGI