SENSITIVE

Description

> Get or Set sensitivity of the motion detection in every channel.

> The CHANNEL=n command has to be set before this URL command. The format of the URL is

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&CHANNEL=n&SENSITIVE=m
> where
> n is the channel ID started from 1 (Channel 1) and the range is from 1~4.
> m is the sensitive value in the range of 0~100. The less value, more sensitivity.

Input Argument

> n (0~100). 100 is the most sensitive and 0 is the least sensitive in motion detection

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> CHANNEL='1'
> SENSITIVE='10'

- Write Operation

> CHANNEL='1'
> SENSITIVE='10'
> or
> ERROR: CHANNEL Value Failed (if CHANNEL is out of range)
> ERROR: SENSITIVE Value Failed (if SENSITIVE is out of range)

Applicability

- WPL Platform : QUAD Encoder Only

Status

> Valid

See Also

> MOTION_ENABLED

Example

- Read Operation

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&CHANNEL=1&SENSITIVE

- Write Operation

> http://ip:port/cgi-bin/quad?USER=Admin&PWD=123456&CHANNEL=1&SENSITIVE=10

Back to

> HOME, QUAD CGI