LAN_HOSTNAME

Description

> Get or Set Host Name in the device. It allows user to access the device by Host name rather IP address. Some networking configurations in user's PC need to be set correctly to use this function.

Input Argument

> Character strings (< 32 Bytes in WPL Decoders), (< 24 Bytes in EPL Decoders)

Attribute

- Write Only in WPL Decoders
- Readable and Writable in EPL Decoders
- On-Fly (except WPL Decoders)

Return of Message

- None in WPL Decoders
- Same as the LAN_HOSTNAME in SYSTEM CGI

Applicability

- WPL Decoder Devices
- EPL Decoder Devices

Status

> Valid

See Also

> HOST(only available in WPL Decoder Devices), LAN_IP, LAN_NETMASK

Example

- Read Operation (Only in EPL Decoder Devices)

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&LAN_HOSTNAME

- Write Operation

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&LAN_HOSTNAME=LocalHost

Back to

> HOME, URL CGI, SYSTEM CGI