V2_WAN_STATUS

Description

> Get the WAN port runtime status. It is similar to WAN_STATUS but not perform the connectivity and DNS test.

> If the CHANNEL=n was set with this URL to the Multi-Channel device, the Router's WAN port runtime status will be returned.

Input Argument

> None

Attribute

- Read Only
- Not On-Fly

Return of Message

> WAN_TYPE='1'
> WAN_IP='192.168.0.100'
> WAN_NETMASK='255.255.255.0'
> WAN_GATEWAY='192.168.0.254'

Applicability

- WPL Platform : All Devices
- EPL Platform : All Devices
- PlatfotmT : All Devices
- Multi-Channel Encoder : All Devices

Status

> Valid

See Also

> WAN, WAN_STATUS, WAN_TYPE, WAN_IP, WAN_NETMASK, WAN_GATEWAY, WAN_PPPOE_USERNAME, WAN_PPPOE_PASSWORD

Example

> http://ip:port/cgi-bin/system?USER=Admin&PWD=123456&V2_WAN_STATUS
> or
> http://ip:port/cgi-bin/cmd/system?V2_WAN_STATUS

Back to

> HOME, SYSTEM CGI