System CGI Program

Only root could set the configuration through this SYSTEM CGI. If the logon user is not root, all write commands will be treated as read commands

List of URLs

URL | Attribute (R/W, On-Fly)1
WPL Platform | EPL Platfrom | Platform T | Multi-Channel Encoder
Encoder | Decoder | Encoder | Decoder | Encoder | Decoder | Router | Video Server
FACTORY_DEFAULT | X,X | X,X | X,X | X,X | X,X | X,X | X,X | X,X
SAVE_REBOOT | X,X | X,X | X,X | X,X | X,X | X,X | X,X | X,X
SAVE | X,X | X,X | X,X | X,X | X,X | X,X | X,X | X,X
REBOOT | X,X | X,X | X,X | X,X | X,X | X,X | X,X | X,X
SYSTEM_INFO | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X
SYSTEM_PROPERTY | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X
WAN | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X
WAN_STATUS | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X
V2_WAN_STATUS | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X
WAN_TYPE | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RO,X
WAN_IP | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RO,X
WAN_NETMASK | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RO,X
WAN_GATEWAY | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RO,X
WAN_PPPOE_USERNAME | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RO,X
WAN_PPPOE_PASSWORD | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RO,X
SPEED_WAN | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
SPEED_LAN | RW,X | RW,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X
LAN | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X
LAN_IP | RW,X | RW,V | None | None | None | None | RO,X | RO,X
LAN_NETMASK | RW,X | RW,V | None | None | None | None | RO,X | RO,X
LAN_HOSTNAME | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
DNS | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X
DNS_PRIMARY | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
DNS_SECONDARY | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
DDNS | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X
DDNS_TYPE | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
DDNS_HOSTNAME | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
DDNS_SERVICE | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
DDNS_USERNAME | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
DDNS_PASSWORD | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
DDNS_CONFIG | None | None | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
DATE | RO,X | None | RO,X | None | RO,X | None | RO,X | RO,X
DATE_TYPE | RW,X | None | RW,V | None | RW,V | None | RW,V | RO,X
DATE_SNTP_IP | RW,X | None | RW,V | None | RW,V | None | RW,V | RO,X
DATE_SNTP_UPDATE | RW,X | None | RW,V | None | RW,V | None | RW,V | RO,X
DATE_MANUAL_DATE | RW,X | None | RW,V | None | RW,V | None | RW,V | RO,X
DATE_MANUAL_TIME | RW,X | None | RW,V | None | RW,V | None | RW,V | RO,X
DATE_MANUAL_ZONE | RW,X | None | RW,V | None | RW,V | None | RW,V | RO,X
DATE_CONFIG | None | None | RW,V | None | RW,V | None | RW,V | RO,X
DAYLIGHT_SAVING_CONFIG | RW,X2 | None | RW,V | None | RW,V | None | RW,V | RO,X
PORT | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X3 | RO,X
PORT_HTTP | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X | RW,X
PORT_SEARCH_1 | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
PORT_SEARCH_2 | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
PORT_SEARCH | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,V | RO,X
PORT_REGISTER | RW,X | None | RO,X | None | RO,X | None | RO,X | RO,X
PORT_CONTROL | RW,X | None | RW,V | None | RW,V | None | RW,V3 | RW,X
PORT_VIDEO | RW,X | None | RW,V | None | RW,V | None | RW,V3 | RW,X
PORT_MULTICAST | RW,X | None | RW,V | None | RW,V | None | RW,V3 | RW,X
V2_PORT_RTSP | RW,X | None | RW,V | None | RW,V | None | RW,V3 | RW,X
V2_PORT_RTP_MULTI_VIDEO | RW,X | None | RW,V | None | RW,V | None | RW,V3 | RW,X
V2_PORT_RTP_MULTI_AUDIO | RW,X | None | RW.V | None | RW,V | None | RW,V3 | RW,X
TOS | RO,X | None | RO,X | None | RO,X | None | RO,X3 | RO,X
VIDEO_TOS_TYPE | RW,X | None | RW,X | None | RW,X | None | RO,X3 | RW,X
VIDEO_TOS_PRIORITY | RW,X | None | RW,X | None | RW,X | None | RO,X3 | RW,X
ACCOUNT | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,X | RO,X
ACCOUNT_ROOT_NAME | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,X | RO,X
ACCOUNT_ROOT_PASSWORD | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,X | RO,X
ACCOUNT_ROOT | None | None | RW,V | RW,V | RW,V | RW,V | RW,X | RO,X
ACCOUNT_USER_NAME_N | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,X | RO,X
ACCOUNT_USER_PASSWORD_N | RW,X | RW,X | RW,V | RW,V | RW,V | RW,V | RW,X | RO,X
ACCOUNT_USER_N | None | None | RW,V | RW,V | RW,V | RW,V | RW,X | RO,X
LOGIN | None | None | RO,X | None | RO,V | None | None | None
LANGUAGE | RW,V | RW,V | RW,V | RW,V | RW,V | RW,V | RW,V | RW,V
VIDEO_TV | RW,X | None | RW,V4 | None | RW,V4 | None | RO,X | RW,V4
VIDEO_FPS | RO,X | None | RO,X | None | RO,X | None | RO,X | RO,X
VIDEO_MULTICAST_TTL | RW,X | None | RW,V | None | RW,V | None | RO,X | RW.X
V2_MULTICAST_IP | RW,X | None | RW,V | None | RW,V | None | RW,X | RW,X4
V2_MUTLICAST_IF | RW,X | RW,X | RO,X | RO,X | RO,X | RO,X | RO,X | RO,X
IGMP_ENABLED | RW,X | None | RW,V | None | RW,V | None | RW,X | RO,X
RTSP_AUTHEN | RW,X2 | None | RW,V | None | RW,V | None | RO,X | RW,X
RTP_B2 | RW,X2 | None | RW,V | None | RW,V | None | RO,X | RW,X
V2_AUDIO_ENABLED | RW,X5 | None | RW,V5 | None | RW,V5 | None | RO,X5 | RW,X5
AUDIO_IN_SENSITIVITY | None | RW,V5 | RW,V5 | RW,V5 | RW,V5 | RW,V5 | RO,X | RW,X5
AUDIO_OUT_VOLUME | None | None | RW,V5 | RW,V5 | RW,V5 | RW,V5 | RO,X | RW,X5
AUDIO_OUT_LEVEL | None | RW,V5 | None | None | None | None | None | None
V2_STREAMING_METHOD | RW,X | None | RW,V | None | RW,X | None | RO,X | RW,X
V2_STREAMING_TYPE | RW,X | None | RO,X | None | RO,X | RO,X | RO,X | RO,X
PROTOCOL_TYPE | RW,X | None | RO,X | None | RO,X | RO,X | RO,X | RO,X
V2_LOWPASS_FILTER | RW,X | None | None | None | None | None | None | None
V2_FAILOVER | RW,X | None | None | None | None | None | None | None
PROFILE_ID | None | None | RO,X | None | None | None | RO,X | RO,X4
ACTIVEX_URL | RO,X | None | RO,X | None | RO,X | None | RO,X | None

Back to

> HOME

Foot Note

1 | The first part is for Access Mode. It could be RW (Readable and Writeable), RO (Read Only), WO (Write Only) or None (Not Support) The second part is for On-Fly indication. if the change of URL is effective immediately without save and reboot, It could be V (the URL is on-fly). Otherwise, it is X (the URL is not on-fly).
2 | Only be available of 1CH Encoder. For 2CH and Quad Encoders, it is not available.
3 | Return the CHANNEL 1 video server's configuration. If the CHANNEL 1 video server does not connect to router, the error message will be returned
4 | Need to check device's specification to know its access attributes. It is helpful to check the VIDEO_TV URL description.
5 | Need to check device's specification to know if there is AudioIn and AudioOut functions