PTZ_VENDOR

Description

> Get or Set the PTZ Vendor and Protocol configurations.

> For IP Camera, this URL is useless and the PTZ Vendor and Protocol were fixed to ACTi. For a Video Server, this URL could get or set the PTZ vendor and protocol of the analog PTZ camera.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's PTZ_VENDOR configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

> The available PTZ Vendors and Protocols were listed below.

> PTZ Vendor | PTZ Protocol
> ACTI | ACTI
> DYNACOLOR | DYNACOLOR
> EYEVIEW | V1
> V2
> GE | ¡@
> HARRISONTECH | ¡@
> KAMPRO | KAMPRO
> LILIN | LILIN
> MESSOA | ¡@
> NICECAM | NICECAM
> PANASONIC | PANASONIC
> PELCO | PELCOD
> PELCOP
> PELCOPV1
> PELCOPV2
> PIXIM | PIXIM
> SAMSUNG | SAMSUNG
> TOA | TOA
> VICOM | VICOM
> VIDEOTREC | VIDEOTREC
> VCL | ¡@
> SONY | VISCA

Input Argument

> n,m where n: PTZ Vendor and m: PTZ Protocol. Refer to above table.

Attribute

- Readable and Writable
- On-Fly

Return of Message

- Read Operation

> OK: PTZ_VENDOR='SONY,VISCA'

- Write Operation

> OK: PTZ_VENDOR='SONY,VISCA'
> or
> ERROR: PTZ_VENDOR='SONY,VISCA'

Applicability

- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : 4CH and 16CH Video Servers

Status

> Valid

See Also

> ADDR, ZOOM, ZOOM_POSITION, FOCUS, FOCUS_POSITION, MOVE, MOVE_LIMIT, MOVE_LIMIT_GET, MOVE_MAX_SPEED_GET, POSITION, POSITION_GET

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&PTZ_VENDOR
> or
> http://ip:port/cgi-bin/cmd/encoder? PTZ_VENDOR

- Write Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&PTZ_VENDOR=SONY,VISCA
> or
> http://ip:port/cgi-bin/cmd/encoder? PTZ_VENDOR=SONY,VISCA

Back to

> HOME, ENCODER CGI