System CGI Program

Encoder CGI Program

Only root could set the configuration through this MPEG4 CGI. If the logon user is not root, all write commands will be treated as read commands. The CGI is only available in the Encoder Devices. The URL in this CGI will be forwarded to all video servers by router in the Multi-Channel Encoder platform.

NOTE:

> This CGI is new CGI for replacing mpeg4 CGI.

List of URLs

URL | Attribute (R/W, On-Fly)1
EPL Platfrom | Platform T | Multi-Channel Encoder2
Encoder | Encoder | Video Server
VIDEO_ENCODER | RW,V | RW,V | RW,V
VIDEO_BITRATE | RW,V | RW,V | RW,V
VIDEO_MAX_BITRATE | RW,V | RW,V | RW,V
VIDEO_RESOLUTION | RW,V | RW,V | RW,V
VIDEO_MJPEG_QUALITY | RW,V | RW,V | RW,V
VIDEO_MPEG4_QUALITY | RW,V | RW,V | RW,V
VIDEO_H264_QUALITY | None | RW,V | None
VIDEO_FPS | RW,V | RW,V | RW,V
VIDEO_FPS_NUM | RW,V | RW,V | RW,V
VIDEO_H264_FPS | None | RW,V | None
VIDEO_MJPEG_FPS | RW,V | RW,V | RW,V
VIDEO_VARIABLE_FPS | WO,V | WO,V | WO,V
VARIABLE_FPS_NUM | RW,V | RW,V | RW,V
MOTION_ENABLED | RW,V | RW,V | RW,V
MOTION_CONFIG | RW,V | RW,V | RW,V
MOTION_CONFIG_GET | RO,X | RO,X | RO,X
MOTION_SENSITIVE | WO,V | WO,V | WO,V3
MOTION_TIMER | WO,V | WO,V | WO,V3
MOTION_OBJ | WO,V | WO,V | WO,V3
DIO_OUTPUT | WO,V | WO,V | WO,V
EVENT_ENABLED | RW,V | RW,V | RW,V
EVENT_PRE_TIME | RW,V | RW,V | RW,V
EVENT_POST_TIME | RW,V | RW,V | RW,V
EVENT_INTERVAL | RW,V | RW,V | RW,V
VIDEO_WB_MODE | RW,V4 | RW,V4 | None
VIDEO_WB_GAIN | RW,V4 | RW,V4 | None
VIDEO_EXPOSURE_MODE | None | None | None
VIDEO_EXPOSURE_GAIN | RW,V4 | RW,V4 | None
VIDEO_SHUTTER_MODE | RW,V4 | RW,V4 | None
VIDEO_SHUTTER_SPEED | RW,V4 | RW,V4 | None
VIDEO_FLICKLESS | RW,V4 | RW,V4 | None
VIDEO_AGC_GAIN | RW,V4 | RW,V4 | None
VIDEO_IRIS | RW,V4 | RW,V4 | None
VIDEO_BLC_MODE | RW,V4 | RW,V4 | None
VIDEO_SENSEUP_LEVEL | RW,V4 | RW,V4 | None
VIDEO_DAYNIGHT_MODE | RW,V4 | RW,V4 | None
VIDEO_MIRROR_MODE | RW,V4 | RW,V4 | None
VIDEO_FLIP_MODE | RW,V4 | RW,V4 | None
VIDEO_MAX_SHUTTER | RW,V4 | RW,V4 | None
LENS_COMPENSATION | RW,V4 | RW,V4 | None
DAY_GAIN_THD | RW,V4 | RW,V4 | None
SNAPSHOT | WO,X | WO,X | WO,X3
CAMERA_PRESET | WO,V4 | WO,V4 | WO,V3,4
ADDR | RW,V4 | RW,V4 | RW,V3,4
PTZ_VENDOR | RW,V4 | RW,V4 | RW,V3,4
ZOOM | WO,V4 | WO,V4 | RO,V3,4
ZOOM_POSITION | RO,V4 | RO,V4 | RO,V3,4
FOCUS | WO,V4 | WO,V4 | WO,V3,4
FOCUS_POSITION | RO,V4 | RO,V4 | RO,V3,4
MOVE | WO,V4 | WO,V4 | WO,V3,4
MOVE_LIMIT | WO,V4 | WO,V4 | WO,V3,4
MOVE_LIMIT_GET | RO,V4 | RO,V4 | RO,V3,4
MOVE_MAX_SPEED_GET | RO,V4 | RO,V4 | RO,V3,4
POSITION | WO,V4 | WO,V4 | WO,V3,4
POSITION_GET | RO,V4 | RO,V4 | RO,V3,4

Back to

> HOME

Foot Note

1 | The first part is for Access Mode. It could be RW (Readable and Writeable), RO (Read Only), WO (Write Only) or None (Not Support) The second part is for On-Fly indication. if the change of URL is effective immediately without save and reboot, It could be V (the URL is on-fly). Otherwise, it is X (the URL is not on-fly).
2 | Only be available of 4CH and 16CH Video Server
3 | Return the CHANNEL 1 video server's configuration. If the CHANNEL 1 video server does not connect to router, the error message will be returned
4 | Need to check device's specification to know its access attributes. It is helpful to check the Camera Setup Design Specification.