VIDEO_BITRATE

Description

> Get or set the average video bitrate in bits/sec for MPEG4/H.264 encoding.

> This URL will not take effect if

> 1. The encoder type is MJPEG (refer to VIDEO_ENCODER)
> 2. The Video Quality is not NONE in MPEG4/H.264 encoding (refer to VIDEO_MPEG4_QUALITY).
> 3. The Maximum Video Bitrate is not unlimited for MPEG4/H.264 encoding (refer to VIDEO_MAX_BITRATE)

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, this command is read-only command and the CHANNEL 1 video server's VIDEO_BITRATE configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> 28K, 56K, 128K, 256K, 384K, 500K, 750K, 1M, 1.2M, 1.5M, 2M, 2.5M, 3M in unit of bits/sec.

Attribute

- Readable and Writable
- On-Fly

Return of Message

-     Read Operation

> OK: VIDEO_BITRATE='3M'

- Write Operation

> OK: VIDEO_BITRATE='3M'
> or
> ERROR: VIDEO_BITRATE='3M'

Applicability

- WPL Platform : All 1CH and 2CH Encoders
- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : All Video Servers

Status

> Valid

See Also

> VIDEO_ENCODER, VIDEO_MAX_BITRATE, VIDEO_MPEG4_QUALITY, VIDEO_H264_QUALITY

Example

- Read Operation

> http://ip:port/cgi-bin/CGI?USER=Admin&PWD=123456&VIDEO_BITRATE
> or
> http://ip:port/cgi-bin/cmd/CGI? VIDEO_BITRATE

> where CGI could be mpeg4 or encoder

- Write Operation

> http://ip:port/cgi-bin/CGI?USER=Admin&PWD=123456&VIDEO_BITRATE=3M
> or
> http://ip:port/cgi-bin/cmd/CGI? VIDEO_BITRATE=3M

> where CGI could be mpeg4 or encoder

Back to

> HOME, MPEG4 CGI, ENCODER CGI