PORT

Description

> Get the device's networking port number configurations.

> The return message of this command is different between WIS and EPL Decoder Device.

Input Argument

> None

Attribute

- Read Only

Return of Message

> From WPL Decoder Devices:

> > PORT_HTTP='80'
> > PORT_HOST_SEARCH_1='6005'
> > PORT_HOST_SEARCH_2='6006'
> > PORT_HOST_SDK_1='10060'
> > PORT_HOST_SDK_2='10061'

> Form EPL Decoder Devices:

> - Not connect to an encoder

> > PORT_HTTP='80'
> > PORT_SEARCH_1='6005'
> > PORT_SEARCH_2='6006'

> - connect to an encoder

> > PORT_HTTP='80'
> > PORT_HOST_SEARCH_1='6005'
> > PORT_HOST_SEARCH_2='6006'
> > PORT_REMOTE_REGISTER='6000'
> > PORT_REMOTE_CONTROL='6001'
> > PORT_REMOTE_VIDEO='6002'
> > PORT_REMOTE_MULTICAST='5000'

> > where the PORT_REMOTE_REGISTER, PORT_REMOTE_CONTROL, PORT_REMOTE_VIDEO, PORT_REMOTE_MULTICAST are the port used in the encoder

Applicability

- WPL Decoder Devices
- EPL Decoder Devices

Status

> Valid

See Also

> PORT_HTTP, PORT_HOST_SEARCH_1, PORT_HOST_SEARCH_2

Example

> http://ip:port/cgi-bin/url.cgi?USER=Admin&PWD=123456&PORT

Back to

> HOME, URL CGI