FOCUS_POSITION

Description

> Get the current FOCUS Position in hexadecimal value.

> If the CHANNEL=n was not set with this URL to the Multi-Channel device, the CHANNEL 1 video server's FOCUS_POSITION configuration will be returned. If the CHANNEL 1 video server does not connect to the router, the error message will be returned.

Input Argument

> None

Attribute

- Read Only
- On-Fly

Return of Message

- Read Operation

> OK: FOCUS_POSITION='0xn'
> where n is in hexadecimal for current focus position.
> or
> ERROR: FOCUS_POSITION

Applicability

- EPL Platform : All Encoders
- PlatfotmT : All Encoders
- Multi-Channel Encoder : 4CH and 16CH Video Servers

Status

> Valid

See Also

> ADDR, PTZ_VENDOR, ZOOM, ZOOM_POSITION, FOCUS, MOVE, MOVE_LIMIT, MOVE_LIMIT_GET, MOVE_MAX_SPEED_GET, POSITION, POSITION_GET

Example

- Read Operation

> http://ip:port/cgi-bin/encoder?USER=Admin&PWD=123456&FOCUS_POSITION
> or
> http://ip:port/cgi-bin/cmd/encoder?FOCUS_POSITION

Back to

> HOME, ENCODER CGI